# Design Rule Verification Report

Date: |  | 04/03/2020
Time: |  | 14:04:56
Elapsed Time: |  | 00:00:01
Filename: |  | K:\Work\Z20X\processors\ez80f91\electronics\PCB.PcbDoc
Warnings: |  | 0
Rule Violations: |  | 0

## Summary

Warnings | Count
--- | ---
Total | 0

Rule Violations | Count
--- | ---
Clearance Constraint (Gap=0.24mm) (All),(All) | 0
Clearance Constraint (Gap=0.35mm) ((IsRegion)),(All) | 0
Short-Circuit Constraint (Allowed=No) (All),(All) | 0
Un-Routed Net Constraint ( (All) ) | 0
Width Constraint (Min=0.2mm) (Max=0.5mm) (Preferred=0.2mm) (All) | 0
Power Plane Connect Rule(Direct Connect )(Expansion=0.5mm) (Conductor Width=0.35mm) (Air Gap=0.35mm) (Entries=4) (All) | 0
Hole Size Constraint (Min=0.025mm) (Max=2.5mm) (Disabled)(All) | 0
Hole To Hole Clearance (Gap=0mm) (Disabled)(All),(All) | 0
Minimum Solder Mask Sliver (Gap=-50mm) (Disabled)(All),(All) | 0
Silk To Solder Mask (Clearance=-50mm) (Disabled)(IsPad),(All) | 0
Silk to Silk (Clearance=-50mm) (Disabled)(All),(All) | 0
Net Antennae (Tolerance=0mm) (Disabled)(All) | 0
Height Constraint (Min=0mm) (Max=25.4mm) (Prefered=12.7mm) (All) | 0
Silk primitive without silk layer | 0
Total | 0